
\chapter{\abstractname}
\singlespacing
\noindent Monitoring Kesehatan Struktur (SHM) secara tradisional membutuhkan banyak sensor dan model yang kompleks, sehingga tidak praktikal untuk pengaplikasian di lapangan. Studi ini menginvestigasi apakah sinyal yang direkam hanya pada sensor ujung atas dan bawah dari kolom-kolom grup sensor cukup untuk memberikan informasi yang akurat pada klasifikasi lokasi kerusakan. Pengujian dilakukan pada dataset QUGS, sebuhah struktur \textit{grid} baja dengan jumlah \textit{node} 6$\times$5 terpasang sensor akselerometer dan digetarkan pada \textit{white noise shaker}. Sinyal getaran dikonversi menjadi fitur frekuensi-waktu menggunakan STFT dan lima algoritma \textit{machine learning} digunakan untuk klasifikasi. Setiap kolom grup dievaluasi dengan \textit{cross-validation} untuk menguji generalisasi model. Hasil menunjukkan bahwa dengan jumlah sensor yang tereduksi, lima algoritma \textit{machine learning} mencapai akurasi klasifikasi lebih dari 90\%. Studi ini menunjukkan bahwa posisi sensor yang strategis dan ekstraksi fitur berbasis STFT cukup untuk mendeteksi lokasi kerusakan secara efektif dan menjadi alternatif yang simpel untuk pendekatan monitoring kesehatan struktur yang kompleks.

\cleardoublepage
\setmainlanguage{english}
\chapter{\abstractname}
\noindent \textit{Structural Health Monitoring (SHM) traditionally requires dense sensor arrays and complex models, which can be impractical for field deployment. This study investigates whether vibration signals captured from only the top and bottom sensors of grouped structural columns retain sufficient information for accurate damage location classification. Experiments are conducted on the QUGS dataset, which represents a 6$\times$5 steel-frame grid structure under controlled laboratory conditions. Vibration signals are converted into time-frequency features using the Short-Time Fourier Transform (STFT), and five classical machine learning algorithms, including Support Vector Machines (SVM), are used for classification. Each vertical column group is evaluated through cross-validation to test generalisation across paths. Results show that even with reduced sensor input, all five algorithms achieve over 90\% classification accuracy. These findings demonstrate that strategic sensor placement and STFT-based features are sufficient to detect structural damage effectively, offering a simple and interpretable alternative to more complex SHM approaches}