@article{abdeljaber2017,
  title = {Real-Time Vibration-Based Structural Damage Detection Using One-Dimensional Convolutional Neural Networks},
  author = {Abdeljaber, Osama and Avci, Onur and Kiranyaz, Serkan and Gabbouj, Moncef and Inman, Daniel J.},
  date = {2017-02},
  journaltitle = {Journal of Sound and Vibration},
  shortjournal = {Journal of Sound and Vibration},
  volume = {388},
  pages = {154--170},
  issn = {0022460X},
  doi = {10.1016/j.jsv.2016.10.043},
  url = {https://linkinghub.elsevier.com/retrieve/pii/S0022460X16306204},
  urldate = {2024-06-19},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\5WG6DL7B\Abdeljaber et al. - 2017 - Real-time vibration-based structural damage detect.pdf}
}

@article{gui2017,
  title = {Data-Driven Support Vector Machine with Optimization Techniques for Structural Health Monitoring and Damage Detection},
  author = {Gui, Guoqing and Pan, Hong and Lin, Zhibin and Li, Yonghua and Yuan, Zhijun},
  date = {2017-02-01},
  journaltitle = {KSCE Journal of Civil Engineering},
  shortjournal = {KSCE Journal of Civil Engineering},
  volume = {21},
  number = {2},
  pages = {523--534},
  issn = {1226-7988},
  doi = {10.1007/s12205-017-1518-5},
  url = {https://www.sciencedirect.com/science/article/pii/S1226798824047913},
  urldate = {2025-09-29},
  abstract = {Rapid detecting damages/defeats in the large-scale civil engineering structures, assessing their conditions and timely decision making are crucial to ensure their health and ultimately enhance the level of public safety. Advanced sensor network techniques recently allow collecting large amounts of data for structural health monitoring and damage detection, while how to effectively interpret these complex sensor data to technical information posts many challenges. This paper presents three optimization-algorithm based support vector machines for damage detection. The optimization algorithms, including grid-search, partial swarm optimization and genetic algorithm, are used to optimize the penalty parameters and Gaussian kernel function parameters. Two types of feature extraction methods in terms of time-series data are selected to capture effective damage characteristics. A benchmark experimental data with the 17 different scenarios in the literature were used for verifying the proposed data-driven methods. Numerical results revealed that all three optimized machine learning methods exhibited significantly improvement in sensitivity, accuracy and effectiveness over conventional methods. The genetic algorithm based SVM had a better prediction than other methods. Two different feature methods used in this study also demonstrated the appropriate features are crucial to improve the sensitivity in detecting damage and assessing structural health conditions. The findings of this study are expected to help engineers to process big data and effectively detect the damage/defects, and thus enable them to make timely decision for supporting civil infrastructure management practices.},
  keywords = {data-driven modeling,optimization,structural health monitoring and damage detection,support vector machine learning},
  file = {C\:\\Users\\damar\\Zotero\\storage\\V8PP7XRS\\Gui et al. - 2017 - Data-driven support vector machine with optimizati.pdf;C\:\\Users\\damar\\Zotero\\storage\\KMM2Q6NT\\S1226798824047913.html}
}

@book{geron2019,
  title = {Hands-on Machine Learning with {{Scikit-Learn}}, {{Keras}}, and {{TensorFlow}}: Concepts, Tools, and Techniques to Build Intelligent Systems},
  shorttitle = {Hands-on Machine Learning with {{Scikit-Learn}}, {{Keras}}, and {{TensorFlow}}},
  author = {Géron, Aurélien},
  date = {2019},
  edition = {Second edition},
  publisher = {O'Reilly},
  location = {Beijing Boston Farnham Sebastopol Tokyo},
  abstract = {Through a series of recent breakthroughs, deep learning has boosted the entire field of machine learning. Now, even programmers who know close to nothing about this technology can use simple, efficient tools to implement programs capable of learning from data. This practical book shows you how. By using concrete examples, minimal theory, and two production-ready Python frameworks--Scikit-Learn and TensorFlow--author Aurélien Géron helps you gain an intuitive understanding of the concepts and tools for building intelligent systems. You'll learn a range of techniques, starting with simple linear regression and progressing to deep neural networks. With exercises in each chapter to help you apply what you've learned, all you need is programming experience to get started. Explore the machine learning landscape, particularly neural nets Use Scikit-Learn to track an example machine-learning project end-to-end Explore several training models, including support vector machines, decision trees, random forests, and ensemble methods Use the TensorFlow library to build and train neural nets Dive into neural net architectures, including convolutional nets, recurrent nets, and deep reinforcement learning Learn techniques for training and scaling deep neural nets},
  isbn = {978-1-4920-3264-9 978-1-4920-3261-8},
  langid = {english},
  pagetotal = {1}
}

@inproceedings{Kohavi1995ASO,
  title={A Study of Cross-Validation and Bootstrap for Accuracy Estimation and Model Selection},
  author={Ron Kohavi},
  booktitle={International Joint Conference on Artificial Intelligence},
  year={1995},
  url={https://api.semanticscholar.org/CorpusID:2702042}
}

@article{JMLR:v9:vandermaaten08a,
  author  = {Laurens van der Maaten and Geoffrey Hinton},
  title   = {Visualizing Data using t-SNE},
  journal = {Journal of Machine Learning Research},
  year    = {2008},
  volume  = {9},
  number  = {86},
  pages   = {2579--2605},
  url     = {http://jmlr.org/papers/v9/vandermaaten08a.html}
}

@article{JMLR:v22:20-1061,
  author  = {Yingfan Wang and Haiyang Huang and Cynthia Rudin and Yaron Shaposhnik},
  title   = {Understanding How Dimension Reduction Tools Work: An Empirical Approach to Deciphering t-SNE, UMAP, TriMap, and PaCMAP for Data Visualization},
  journal = {Journal of Machine Learning Research},
  year    = {2021},
  volume  = {22},
  number  = {201},
  pages   = {1-73},
  url     = {http://jmlr.org/papers/v22/20-1061.html}
}

@article{CC01a,
 author = {Chang, Chih-Chung and Lin, Chih-Jen},
 title = {{LIBSVM}: A library for support vector machines},
 journal = {ACM Transactions on Intelligent Systems and Technology},
 volume = {2},
 issue = {3},
 year = {2011},
 pages = {27:1--27:27},
 note =	 {Software available at \url{http://www.csie.ntu.edu.tw/~cjlin/libsvm}}
}

@inproceedings{Hsu2009APG,
  title={A Practical Guide to Support Vector Classification},
  author={Chih-Wei Hsu and Chih-Chung Chang and Chih-Jen Lin},
  year={2009},
  url={https://api.semanticscholar.org/CorpusID:267925897}
}

@article{hsu2002,
  title = {A Comparison of Methods for Multiclass Support Vector Machines},
  author = {Hsu, Chih-Wei and Lin, Chih-Jen},
  date = {2002},
  journaltitle = {IEEE transactions on neural networks},
  shortjournal = {IEEE Trans Neural Netw},
  volume = {13},
  number = {2},
  eprint = {18244442},
  eprinttype = {pmid},
  pages = {415--425},
  issn = {1045-9227},
  doi = {10.1109/72.991427},
  abstract = {Support vector machines (SVMs) were originally designed for binary classification. How to effectively extend it for multiclass classification is still an ongoing research issue. Several methods have been proposed where typically we construct a multiclass classifier by combining several binary classifiers. Some authors also proposed methods that consider all classes at once. As it is computationally more expensive to solve multiclass problems, comparisons of these methods using large-scale problems have not been seriously conducted. Especially for methods solving multiclass SVM in one step, a much larger optimization problem is required so up to now experiments are limited to small data sets. In this paper we give decomposition implementations for two such "all-together" methods. We then compare their performance with three methods based on binary classifications: "one-against-all," "one-against-one," and directed acyclic graph SVM (DAGSVM). Our experiments indicate that the "one-against-one" and DAG methods are more suitable for practical use than the other methods. Results also show that for large problems methods by considering all data at once in general need fewer support vectors.},
  langid = {english}
}

@article{JMLR:v18:16-174,
  title = {Empirical Evaluation of Resampling Procedures for Optimising {{SVM}} Hyperparameters},
  author = {Wainer, Jacques and Cawley, Gavin},
  date = {2017},
  journaltitle = {Journal of Machine Learning Research},
  volume = {18},
  number = {15},
  pages = {1--35},
  url = {http://jmlr.org/papers/v18/16-174.html}
}


@article{diao2023,
  title = {Structural Damage Identification Based on Variational Mode Decomposition–{{Hilbert}} Transform and {{CNN}}},
  author = {Diao, Yansong and Lv, Jianda and Wang, Qiuxiao and Li, Xingjian and Xu, Jing},
  date = {2023-10},
  journaltitle = {Journal of Civil Structural Health Monitoring},
  shortjournal = {J Civil Struct Health Monit},
  volume = {13},
  number = {6--7},
  pages = {1415--1429},
  issn = {2190-5452, 2190-5479},
  doi = {10.1007/s13349-023-00715-3},
  url = {https://link.springer.com/10.1007/s13349-023-00715-3},
  urldate = {2025-05-19},
  langid = {english},
}

@article{zhao2019,
  title = {Bolt Loosening Angle Detection Technology Using Deep Learning},
  author = {Zhao, Xuefeng and Zhang, Yang and Wang, Niannian},
  date = {2019-01},
  journaltitle = {Structural Control and Health Monitoring},
  shortjournal = {Struct Control Health Monit},
  volume = {26},
  number = {1},
  pages = {e2292},
  issn = {15452255},
  doi = {10.1002/stc.2292},
  url = {https://onlinelibrary.wiley.com/doi/10.1002/stc.2292},
  urldate = {2025-05-16},
  langid = {english}
}

@article{abdelwahab1999,
  title = {{{PARAMETERIZATION OF DAMAGE IN REINFORCED CONCRETE STRUCTURES USING MODEL UPDATING}}},
  author = {Abdel Wahab, M.M. and De Roeck, G. and Peeters, B.},
  date = {1999-12},
  journaltitle = {Journal of Sound and Vibration},
  shortjournal = {Journal of Sound and Vibration},
  volume = {228},
  number = {4},
  pages = {717--730},
  issn = {0022460X},
  doi = {10.1006/jsvi.1999.2448},
  url = {https://linkinghub.elsevier.com/retrieve/pii/S0022460X99924483},
  urldate = {2024-12-29},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\P7FDZX9J\abdelwahab1999.pdf.pdf}
}

@article{avci2021,
  title = {A Review of Vibration-Based Damage Detection in Civil Structures: {{From}} Traditional Methods to {{Machine Learning}} and {{Deep Learning}} Applications},
  shorttitle = {A Review of Vibration-Based Damage Detection in Civil Structures},
  author = {Avci, Onur and Abdeljaber, Osama and Kiranyaz, Serkan and Hussein, Mohammed and Gabbouj, Moncef and Inman, Daniel J.},
  date = {2021-01-15},
  journaltitle = {Mechanical Systems and Signal Processing},
  shortjournal = {Mechanical Systems and Signal Processing},
  volume = {147},
  pages = {107077},
  issn = {0888-3270},
  doi = {10.1016/j.ymssp.2020.107077},
  url = {https://www.sciencedirect.com/science/article/pii/S0888327020304635},
  urldate = {2025-05-09},
  abstract = {Monitoring structural damage is extremely important for sustaining and preserving the service life of civil structures. While successful monitoring provides resolute and staunch information on the health, serviceability, integrity and safety of structures; maintaining continuous performance of a structure depends highly on monitoring the occurrence, formation and propagation of damage. Damage may accumulate on structures due to different environmental and human-induced factors. Numerous monitoring and detection approaches have been developed to provide practical means for early warning against structural damage or any type of anomaly. Considerable effort has been put into vibration-based methods, which utilize the vibration response of the monitored structure to assess its condition and identify structural damage. Meanwhile, with emerging computing power and sensing technology in the last decade, Machine Learning (ML) and especially Deep Learning (DL) algorithms have become more feasible and extensively used in vibration-based structural damage detection with elegant performance and often with rigorous accuracy. While there have been multiple review studies published on vibration-based structural damage detection, there has not been a study where the transition from traditional methods to ML and DL methods are described and discussed. This paper aims to fulfill this gap by presenting the highlights of the traditional methods and provide a comprehensive review of the most recent applications of ML and DL algorithms utilized for vibration-based structural damage detection in civil structures.},
  keywords = {Artificial Neural Networks,Civil infrastructure,Deep Learning,Infrastructure health,Machine Learning,Structural damage detection,Structural Health Monitoring,Vibration-based methods},
  file = {C\:\\Users\\damar\\Zotero\\storage\\59EASW6K\\Avci et al. - 2021 - A review of vibration-based damage detection in ci.pdf;C\:\\Users\\damar\\Zotero\\storage\\GQZUKPQN\\10.1016@j.ymssp.2020.107077.pdf.pdf}
}

@inproceedings{van2020,
  title = {Statistical {{Feature Extraction}} in {{Machine Fault Detection}} Using {{Vibration Signal}}},
  booktitle = {2020 {{International Conference}} on {{Information}} and {{Communication Technology Convergence}} ({{ICTC}})},
  author = {Van, Bui and Van Hoa, Nguyen and Nguyen, Huy and Jang, Yeong Min},
  date = {2020-10},
  pages = {666--669},
  issn = {2162-1233},
  doi = {10.1109/ICTC49870.2020.9289285},
  url = {https://ieeexplore.ieee.org/document/9289285/figures#figures},
  urldate = {2024-08-26},
  abstract = {Gearbox faults are one of the most common types in the industrial factory environment. Early detection of these faults allows fast replacement rather than a costly emergency. Nowadays, early machine fault detection application is improving due to the improvement of the IoT network and real-time analysis. The vibration signal is collected from Spectra Quest's Gearbox Prognostics Simulator and analyzed for fault classification. The preprocessing includes fast Fourier transform and statistical feature extraction. The AI algorithms are Artificial Neural Network, Logistic Regression, and Support Vector Machine. The highest accuracy reached is 100\%.},
  eventtitle = {2020 {{International Conference}} on {{Information}} and {{Communication Technology Convergence}} ({{ICTC}})},
  keywords = {ANN,Fault detection,Feature extraction,LR,Machine Learning,Manufacturing,Production facilities,Real-time systems,Support vector machines,SVM,Vibration Signal,Vibrations},
  file = {C\:\\Users\\damar\\Zotero\\storage\\TW69QG8K\\van2020.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\AZM769D7\\figures.html}
}

@article{katam2025,
  title = {Machine Learning-Driven Structural Health Monitoring: {{STFT-based}} Feature Extraction for Damage Detection},
  shorttitle = {Machine Learning-Driven Structural Health Monitoring},
  author = {Katam, Rakesh and Pasupuleti, Venkata Dilip Kumar and Kalapatapu, Prafulla},
  date = {2025-08},
  journaltitle = {Structures},
  shortjournal = {Structures},
  volume = {78},
  pages = {109244},
  issn = {23520124},
  doi = {10.1016/j.istruc.2025.109244},
  url = {https://linkinghub.elsevier.com/retrieve/pii/S2352012425010586},
  urldate = {2025-06-05},
  abstract = {Structural health monitoring (SHM) is essential for ensuring the safety and durability of engineering structures by enabling early identification of damage. This research presents a novel approach that integrates experimental testing, signal processing, and machine learning to enhance damage detection in cantilever beams, mainly when working with limited datasets. Vibration-based time-series data (VBTSD) are gathered from damaged and un­ damaged beams, utilizing fast fourier transform (FFT) and short-time fourier transform (STFT) for frequencydomain analysis. While FFT delivers a comprehensive spectral overview, STFT provides a focused timefrequency analysis, effectively capturing transient structural changes that are critical for early damage detec­ tion. To manage the high-dimensional STFT feature space, an autoencoder is utilized to extract compressed yet informative representations while preserving essential frequency-magnitude variations. The resulting encoded features are then used to train a support vector machine (SVM) classifier, achieving an impressive 98 \% accuracy in predicting the presence of structural damage. The proposed framework is designed to function effectively even with limited data availability, ensuring robustness in real-world SHM applications where data collection is often restricted. The high-resolution frequency selectivity offered by STFT surpasses traditional methods such as wavelet transforms and standalone FFT, making it exceptionally suitable for real-time damage detection. This research highlights the combination of vibration-based feature extraction and machine learning, resulting in a scalable, data-efficient, and computationally feasible approach for SHM. The results aid in the progression of automated damage classification, presenting a practical and dependable resource to improve structural resilience and safety within civil engineering applications.},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\U2WHH4SL\Katam et al. - 2025 - Machine learning-driven structural health monitori.pdf}
}


@inproceedings{bulut2005,
  title = {Real-Time Nondestructive Structural Health Monitoring Using Support Vector Machines and Wavelets},
  author = {Bulut, Ahmet and Singh, Ambuj K. and Shin, Peter and Fountain, Tony and Jasso, Hector and Yan, Linjun and Elgamal, Ahmed},
  editor = {Meyendorf, Norbert and Baaklini, George Y. and Michel, Bernd},
  date = {2005-05-09},
  pages = {180},
  location = {San Diego, CA},
  doi = {10.1117/12.597685},
  url = {http://proceedings.spiedigitallibrary.org/proceeding.aspx?doi=10.1117/12.597685},
  urldate = {2024-04-09},
  eventtitle = {Nondestructive {{Evaulation}} for {{Health Monitoring}} and {{Diagnostics}}},
  file = {C:\Users\damar\Zotero\storage\PUABA5V7\bulut2005.pdf.pdf}
}

@article{caselles2022,
  title = {Estimators for {{Structural Damage Detection Using Principal Component Analysis}}},
  author = {Caselles, Oriol and Martín, Alejo and Vargas-Alzate, Yeudy F. and Gonzalez-Drigo, Ramon and Clapés, Jaume},
  date = {2022-09},
  journaltitle = {Heritage},
  volume = {5},
  number = {3},
  pages = {1805--1818},
  publisher = {Multidisciplinary Digital Publishing Institute},
  issn = {2571-9408},
  doi = {10.3390/heritage5030093},
  url = {https://www.mdpi.com/2571-9408/5/3/93},
  urldate = {2024-05-07},
  abstract = {Structural damage detection is an important issue in conservation. In this research, principal component analysis (PCA) has been applied to the temporal variation of modal frequencies obtained from a dynamic test of a scaled steel structure subjected to different damages and different temperatures. PCA has been applied in order to reduce, as much as possible, the number of variables involved in the problem of structural damage detection. The aim of the PCA study is to determine the minimum number of principal components necessary to explain all the modal frequency variation. Three estimators have been studied: T2 (the square of the vector norm of the projection in the principal component plan), Q (the square of the norm of the residual vector), and the variance explained. In the study, the results related to the undamaged structure needed one principal component to explain the modal frequency variation. However, the high damage configurations need five principal components to explain the modal frequency. The T2 and Q estimators have been arranged in order of increasing damage for all the performed experimental tests. The results indicate that these estimators could be useful to detect damage and to distinguish among a range of intensities of structural damage.},
  issue = {3},
  langid = {english},
  keywords = {ambient temperature,damage configuration,historical structure,monitoring,non-destructive inspection,PCA},
  file = {C:\Users\damar\Zotero\storage\IWTRCID3\Caselles et al. - 2022 - Estimators for Structural Damage Detection Using P.pdf}
}

@article{chen2017,
  title = {Self-{{Loosening Failure Analysis}} of {{Bolt Joints}} under {{Vibration}} Considering the {{Tightening Process}}},
  author = {Chen, Yan and Gao, Qiang and Guan, Zhenqun},
  date = {2017},
  journaltitle = {Shock and Vibration},
  shortjournal = {Shock and Vibration},
  volume = {2017},
  pages = {1--15},
  issn = {1070-9622, 1875-9203},
  doi = {10.1155/2017/2038421},
  url = {https://www.hindawi.com/journals/sv/2017/2038421/},
  urldate = {2025-05-16},
  abstract = {By considering the tightening process, a three-dimensional elastic finite element analysis is conducted to explore the mechanism of bolt self-loosening under transverse cyclic loading. According to the geometrical features of the thread, a hexahedral meshing is implemented by modifying the node coordinates based on cylinder meshes and an ABAQUS plug-in is made for parametric modeling. The accuracy of the finite element model is verified and validated by comparison with the analytical and experimental results on torque-tension relationship. And, then, the fastening states acquired by different means are compared. The results show that the tightening process cannot be replaced by a simplified method because its fastening state is different from the real process. With combining the tightening and self-loosening processes, this paper utilizes the relative rotation angles and velocities to investigate the slip states on contact surfaces instead of the Coulomb friction coefficient method, which is used in most previous researches. By contrast, this method can describe the slip states in greater detail. In addition, the simulation result reveals that there exists a creep slip phenomenon at contact surface, which causes the bolt self-loosening to occur even when some contact facets are stuck.},
  langid = {english},
  file = {C\:\\Users\\damar\\Zotero\\storage\\CHXWJ6ZF\\chen2017.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\EGAVQZ32\\Chen et al. - 2017 - Self-Loosening Failure Analysis of Bolt Joints und.pdf}
}

@article{cortes1995,
  title = {Support-Vector Networks},
  author = {Cortes, Corinna and Vapnik, Vladimir},
  date = {1995-09-01},
  journaltitle = {Machine Learning},
  shortjournal = {Mach Learn},
  volume = {20},
  number = {3},
  pages = {273--297},
  issn = {1573-0565},
  doi = {10.1007/BF00994018},
  url = {https://doi.org/10.1007/BF00994018},
  urldate = {2024-05-07},
  abstract = {Thesupport-vector network is a new learning machine for two-group classification problems. The machine conceptually implements the following idea: input vectors are non-linearly mapped to a very high-dimension feature space. In this feature space a linear decision surface is constructed. Special properties of the decision surface ensures high generalization ability of the learning machine. The idea behind the support-vector network was previously implemented for the restricted case where the training data can be separated without errors. We here extend this result to non-separable training data.},
  langid = {english},
  keywords = {efficient learning algorithms,neural networks,pattern recognition,polynomial classifiers,radial basis function classifiers},
  file = {C\:\\Users\\damar\\Zotero\\storage\\5W2CFHWN\\Cortes and Vapnik - 1995 - Support-vector networks.pdf;C\:\\Users\\damar\\Zotero\\storage\\9BK8NS3K\\cortes1995.pdf.pdf}
}

@online{duval2017,
  title = {Answer to "{{Can STFT}} ({{Short-time Fourier Transform}} ) Be More Useful than {{FFT}} for Analyzing Stationary Signals under Some Circumstances?"},
  shorttitle = {Answer to "{{Can STFT}} ({{Short-time Fourier Transform}} ) Be More Useful than {{FFT}} for Analyzing Stationary Signals under Some Circumstances?},
  author = {Duval, Laurent},
  date = {2017-10-04},
  url = {https://dsp.stackexchange.com/a/44145},
  urldate = {2025-04-26},
  organization = {Signal Processing Stack Exchange},
  file = {C:\Users\damar\Zotero\storage\VKABC5YA\can-stft-short-time-fourier-transform-be-more-useful-than-fft-for-analyzing-s.html}
}

@article{eraliev2022,
  title = {Vibration-{{Based Loosening Detection}} of a {{Multi-Bolt Structure Using Machine Learning Algorithms}}},
  author = {Eraliev, Oybek and Lee, Kwang-Hee and Lee, Chul-Hee},
  date = {2022-01},
  journaltitle = {Sensors},
  volume = {22},
  number = {3},
  pages = {1210},
  publisher = {Multidisciplinary Digital Publishing Institute},
  issn = {1424-8220},
  doi = {10.3390/s22031210},
  url = {https://www.mdpi.com/1424-8220/22/3/1210},
  urldate = {2024-05-10},
  abstract = {Since artificial intelligence (AI) was introduced into engineering fields, it has made many breakthroughs. Machine learning (ML) algorithms have been very commonly used in structural health monitoring (SHM) systems in the last decade. In this study, a vibration-based early stage of bolt loosening detection and identification technique is proposed using ML algorithms, for a motor fastened with four bolts (M8 × 1.5) to a stationary support. First, several cases with fastened and loosened bolts were established, and the motor was operated in three different types of working condition (800 rpm, 1000 rpm, and 1200 rpm), in order to obtain enough vibration data. Second, for feature extraction of the dataset, the short-time Fourier transform (STFT) method was performed. Third, different types of classifier of ML were trained, and a new test dataset was applied to evaluate the performance of the classifiers. Finally, the classifier with the greatest accuracy was identified. The test results showed that the capability of the classifier was satisfactory for detecting bolt loosening and identifying which bolt or bolts started to lose their preload in each working condition. The identified classifier will be implemented for online monitoring of the early stage of bolt loosening of a multi-bolt structure in future works.},
  issue = {3},
  langid = {english},
  keywords = {bolt loosening,bolt-loosening identification,loosening detection,machine learning,signal processing,vibration},
  file = {C\:\\Users\\damar\\Zotero\\storage\\QZSXUW39\\sensors-22-01210-with-cover.pdf;C\:\\Users\\damar\\Zotero\\storage\\T7TG2XEK\\Eraliev et al. - 2022 - Vibration-Based Loosening Detection of a Multi-Bol.pdf}
}

@inproceedings{ganga2022,
  title = {{{SVM Based Vibration Analysis}} for {{Effective Classification}} of {{Machine Conditions}}},
  booktitle = {International {{Congress}} and {{Workshop}} on {{Industrial AI}} 2021},
  author = {Ganga, D. and Ramachandran, V.},
  editor = {Karim, Ramin and Ahmadi, Alireza and Soleimanmeigouni, Iman and Kour, Ravdeep and Rao, Raj},
  date = {2022},
  pages = {415--423},
  publisher = {Springer International Publishing},
  location = {Cham},
  doi = {10.1007/978-3-030-93639-6_36},
  abstract = {In condition monitoring, alarms have been the significant references for assessment of critical conditions. Generation of false alarms or suppression of defectiveness have often occurred while maintenance of machines due to incorrect setting of alarms appropriate to machine conditions. The evolution of data analytics and related technologies for real-time data acquisition as per industrial 4.0 standards will resolve such deceptive problems perceived till date. This paper attempts to elucidate a framework for identification and classification of vibration thresholds as per machine conditions using Internet of Things (IoT) based data acquisition and vibration analytics using support vector machines. The classification algorithm for the detection of higher vibrating range of machines has been tested with different sets of vibration features extracted. Incorporation of IoT devices facilitate unbounded and flexible data acquisition for carrying out detailed analytics in cloud environment. The kernel based support vector machine classifies the features extracted from signal processing into higher and lower vibrating levels of machine and fixes the higher vibration levels as thresholds for condition monitoring. The proposed alarm fixation model automatically classifies the maximum vibrating ranges of machines under different operating conditions. This automated condition monitoring model illustrates the efficacy of cloud environment for execution of exhaustive machine learning algorithms for condition monitoring. The performance analysis of the proposed model on the extracted vibration features validates the competence of machine learning algorithms for precise fixation of vibration thresholds and classification of machine conditions for effective maintenance.},
  isbn = {978-3-030-93639-6},
  langid = {english}
}

@incollection{garrett2020,
  title = {String {{Theory}}},
  booktitle = {Understanding {{Acoustics}}: {{An Experimentalist}}’s {{View}} of {{Sound}} and {{Vibration}}},
  author = {Garrett, Steven L.},
  editor = {Garrett, Steven L.},
  date = {2020},
  pages = {133--178},
  publisher = {Springer International Publishing},
  location = {Cham},
  doi = {10.1007/978-3-030-44787-8_3},
  url = {https://doi.org/10.1007/978-3-030-44787-8_3},
  urldate = {2025-05-09},
  abstract = {The vibrating string has been employed by nearly every human culture to create musical instruments. Although the musical application has attracted the attention of mathematical and scientific analysts since the time of Pythagoras (570~BC–495~BC), we will study the string primarily because its vibrations are easy to visualize and string vibrations introduce concepts and techniques that will recur throughout our study of the vibration and the acoustics of continua. In this chapter, we will develop continuous mathematical functions of position and time that describe the shape of the entire string. The amplitude of such functions will describe the transverse displacement from equilibrium, y(x,\,t), at all positions along the string. The importance of boundary conditions at the ends of strings will be emphasized, and techniques to accommodate both ideal and “imperfect” boundary conditions will be introduced. Solutions that result in all parts of the string oscillating at the same frequency which satisfy the boundary conditions are called normal modes, and the calculation of those normal mode frequencies will be a focus of this chapter.},
  isbn = {978-3-030-44787-8},
  langid = {english},
  keywords = {Harmonic series,Normal modes,Radiation impedance,Standing waves,Transcendental equations,Traveling waves},
  file = {C:\Users\damar\Zotero\storage\PKXH58D2\Garrett - 2020 - String Theory.pdf}
}

@incollection{giurgiutiu2020,
  title = {17 - {{Structural}} Health Monitoring ({{SHM}}) of Aerospace Composites},
  booktitle = {Polymer {{Composites}} in the {{Aerospace Industry}} ({{Second Edition}})},
  author = {Giurgiutiu, Victor},
  editor = {Irving, Philip and Soutis, Constantinos},
  date = {2020-01-01},
  series = {Woodhead {{Publishing Series}} in {{Composites Science}} and {{Engineering}}},
  pages = {491--558},
  publisher = {Woodhead Publishing},
  doi = {10.1016/B978-0-08-102679-3.00017-4},
  url = {https://www.sciencedirect.com/science/article/pii/B9780081026793000174},
  urldate = {2025-05-09},
  abstract = {The chapter deals with structural health monitoring (SHM) of aerospace composites. After a brief introduction, the discussion focuses on the significant types of aerospace composite damage, which is substantially different from the damage usually encountered in aerospace metallic structures. Tension, compression, fastener holes, impact, fatigue damage types are discussed. Damage in composite sandwich structures and adhesive composite joints are also reviewed. The chapter continues with a presentation of the major sensor classes used in SHM practice with focus on advanced sensors, such as optical fiber Bragg gratings (FBG) and piezoelectric wafer active sensors (PWAS). Electrical sensing methods for composites SHM are also discussed. The last part of the chapter discusses the methods of SHM implementation, such as passive sensing SHM, active sensing SHM, local-area sensing with the electromechanical impedance spectroscopy (EMIS), active sensing SHM with electrical methods, and direct methods for impact damage detection. The chapter finishes with a summary, conclusion, and suggestions for further work.},
  isbn = {978-0-08-102679-3},
  keywords = {Active SHM,Aerospace composites,Barely visible damage,Barely visible impact damage,BVD,BVID,Composite damage,Damage detection,Electrical SHM,Electromechanical impedance spectroscopy,EMIS,FBG,Fiber Bragg gratings,Impact damage,Impact detection,Optical sensors,Passive SHM,Piezoelectric wafer active sensors,PWAS,SHM,Structural health monitoring},
  file = {C:\Users\damar\Zotero\storage\NYTBVDQN\Giurgiutiu - 2020 - 17 - Structural health monitoring (SHM) of aerospa.pdf}
}

@article{gomez-cabrera2022,
  title = {Review of {{Machine-Learning Techniques Applied}} to {{Structural Health Monitoring Systems}} for {{Building}} and {{Bridge Structures}}},
  author = {Gomez-Cabrera, Alain and Escamilla-Ambrosio, Ponciano Jorge},
  date = {2022-01},
  journaltitle = {Applied Sciences},
  volume = {12},
  number = {21},
  pages = {10754},
  publisher = {Multidisciplinary Digital Publishing Institute},
  issn = {2076-3417},
  doi = {10.3390/app122110754},
  url = {https://www.mdpi.com/2076-3417/12/21/10754},
  urldate = {2024-05-07},
  abstract = {This review identifies current machine-learning algorithms implemented in building structural health monitoring systems and their success in determining the level of damage in a hierarchical classification. The integration of physical models, feature extraction techniques, uncertainty management, parameter estimation, and finite element model analysis are used to implement data-driven model detection systems for SHM system design. A total of 68 articles using ANN, CNN and SVM, in combination with preprocessing techniques, were analyzed corresponding to the period 2011–2022. The application of these techniques in structural condition monitoring improves the reliability and performance of these systems.},
  issue = {21},
  langid = {english},
  keywords = {building structures,data-based model,machine learning,physics-based model,structural health monitoring},
  file = {C:\Users\damar\Zotero\storage\SAYFD8LC\Gomez-Cabrera and Escamilla-Ambrosio - 2022 - Review of Machine-Learning Techniques Applied to S.pdf}
}

@article{goyal2016,
  title = {The {{Vibration Monitoring Methods}} and {{Signal Processing Techniques}} for {{Structural Health Monitoring}}: {{A Review}}},
  shorttitle = {The {{Vibration Monitoring Methods}} and {{Signal Processing Techniques}} for {{Structural Health Monitoring}}},
  author = {Goyal, D. and Pabla, B. S.},
  date = {2016-12},
  journaltitle = {Archives of Computational Methods in Engineering},
  shortjournal = {Arch Computat Methods Eng},
  volume = {23},
  number = {4},
  pages = {585--594},
  issn = {1134-3060, 1886-1784},
  doi = {10.1007/s11831-015-9145-0},
  url = {http://link.springer.com/10.1007/s11831-015-9145-0},
  urldate = {2024-04-09},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\5862GKAP\goyal2015.pdf.pdf}
}

@article{hassani2023,
  title = {A {{Systematic Review}} of {{Advanced Sensor Technologies}} for {{Non-Destructive Testing}} and {{Structural Health Monitoring}}},
  author = {Hassani, Sahar and Dackermann, Ulrike},
  date = {2023-01},
  journaltitle = {Sensors},
  volume = {23},
  number = {4},
  pages = {2204},
  publisher = {Multidisciplinary Digital Publishing Institute},
  issn = {1424-8220},
  doi = {10.3390/s23042204},
  url = {https://www.mdpi.com/1424-8220/23/4/2204},
  urldate = {2024-05-07},
  abstract = {This paper reviews recent advances in sensor technologies for non-destructive testing (NDT) and structural health monitoring (SHM) of civil structures. The article is motivated by the rapid developments in sensor technologies and data analytics leading to ever-advancing systems for assessing and monitoring structures. Conventional and advanced sensor technologies are systematically reviewed and evaluated in the context of providing input parameters for NDT and SHM systems and for their suitability to determine the health state of structures. The presented sensing technologies and monitoring systems are selected based on their capabilities, reliability, maturity, affordability, popularity, ease of use, resilience, and innovation. A significant focus is placed on evaluating the selected technologies and associated data analytics, highlighting limitations, advantages, and disadvantages. The paper presents sensing techniques such as fiber optics, laser vibrometry, acoustic emission, ultrasonics, thermography, drones, microelectromechanical systems (MEMS), magnetostrictive sensors, and next-generation technologies.},
  issue = {4},
  langid = {english},
  keywords = {advanced sensor technologies,damage identification methods,machine learning,non-destructive evaluation,non-destructive testing,structural health monitoring},
  file = {C:\Users\damar\Zotero\storage\JIPPVCWI\Hassani and Dackermann - 2023 - A Systematic Review of Advanced Sensor Technologie.pdf}
}

@article{hsu,
  title = {A {{Practical Guide}} to {{Support Vector Classiﬁcation}}},
  author = {Hsu, Chih-Wei and Chang, Chih-Chung and Lin, Chih-Jen},
  abstract = {The support vector machine (SVM) is a popular classification technique. However, beginners who are not familiar with SVM often get unsatisfactory results since they miss some easy but significant steps. In this guide, we propose a simple procedure which usually gives reasonable results.},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\3D5K3FV4\Hsu et al. - A Practical Guide to Support Vector Classiﬁcation.pdf}
}

@inproceedings{j.h.park2015,
  title = {Image-Based {{Bolt-loosening Detection Technique}} of {{Bolt Joint}} in {{Steel Bridges}}},
  author = {{J. H. Park} and {T. H. Kim} and {J. T. Kim}},
  date = {2015},
  url = {https://api.semanticscholar.org/CorpusID:36521104},
  abstract = {This paper presents a novel bolt-loosening detection technique using image information of bolted joints in steel bridges. Firstly, existing bolt-loosening detection techniques are reviewed and their benefits and limitations are analyzed. Secondly, a bolt-loosening detection algorithm using image processing techniques is newly proposed for bolted joints in steel bridges. It consists of 3 steps: (1) taking a picture for a bolt joint, (2) segmenting the image to identify a splice plate and each nut, and (3) identifying rotation angle of each nut and detecting boltloosening. As a key technique, the Hough transform is used to identify rotation angles of nuts, and then boltloosening is detected by comparing the angles before and after bolt-loosening. Finally, the applicability of the proposed technique is evaluated by experimental tests with bolt-loosening scenarios. A bolted joint model which consists of a splice plate and 8 sets of bolts and nuts with 2×4 array is used for the tests.}
}

@article{jang2023,
  title = {Vibration Data Feature Extraction and Deep Learning-Based Preprocessing Method for Highly Accurate Motor Fault Diagnosis},
  author = {Jang, Jun-Gyo and Noh, Chun-Myoung and Kim, Sung-Soo and Shin, Sung-Chul and Lee, Soon-Sup and Lee, Jae-Chul},
  date = {2023-01-11},
  journaltitle = {Journal of Computational Design and Engineering},
  volume = {10},
  number = {1},
  pages = {204--220},
  issn = {2288-5048},
  doi = {10.1093/jcde/qwac128},
  url = {https://academic.oup.com/jcde/article/10/1/204/6880159},
  urldate = {2024-09-11},
  abstract = {Abstract             The environmental regulations on vessels being strengthened by the International Maritime Organization has led to a steady growth in the eco-friendly ship market. Related research is being actively conducted, including many studies on the maintenance and predictive maintenance of propulsion systems (including electric motors and rotating bodies) in electric propulsion vessels. The present study intends to enhance the artificial intelligence (AI)-based failure-diagnosis rate for electric propulsion vessel propulsion systems. To verify the proposed AI-based failure diagnosis algorithm for electric motors, this study utilized the vibration data of mechanical equipment (electric motors) in an urban railway station. Securing and preprocessing high-quality data is crucial for improving the failure-diagnosis rate, in addition to the performance of the diagnostic algorithm. However, the conventional wavelet transform method, which is generally used for machine signal processing, has a disadvantage of data loss when the data distribution is abnormal or skewed. This study, to overcome this shortcoming, proposes an AI-based denoising auto encoder (DAE) method that can remove noise while maintaining data characteristics for signal processing of mechanical equipment. This study preprocessed vibration data by using the DAE method, and extracted significant features from the data through the feature extraction method. The extracted features were utilized to train the one-class support vector machine model and to allow the model to diagnose the failure. Finally, the F-1 score was calculated by using the failure diagnosis results, and the most meaningful feature extraction method was determined for the vibration data. In addition, this study compared and evaluated the preprocessing performance based on the DAE and the wavelet transform methods.},
  langid = {english},
  file = {C\:\\Users\\damar\\Zotero\\storage\\H9L6XB8D\\Jang et al. - 2023 - Vibration data feature extraction and deep learnin.pdf;C\:\\Users\\damar\\Zotero\\storage\\WA37YR8L\\Jang et al. - 2023 - Vibration data feature extraction and deep learnin.pdf}
}

@article{kumar2017,
  title = {Time-Frequency Analysis and Support Vector Machine in Automatic Detection of Defect from Vibration Signal of Centrifugal Pump},
  author = {Kumar, Anil and Kumar, Rajesh},
  date = {2017-10},
  journaltitle = {Measurement},
  shortjournal = {Measurement},
  volume = {108},
  pages = {119--133},
  issn = {02632241},
  doi = {10.1016/j.measurement.2017.04.041},
  url = {https://linkinghub.elsevier.com/retrieve/pii/S0263224117302750},
  urldate = {2024-03-18},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\B8JSREBK\kumar2017.pdf.pdf}
}

@incollection{liu2022,
  title = {Hardware {{Acceleration}} for {{1D-CNN Based Real-Time Edge Computing}}},
  booktitle = {Network and {{Parallel Computing}}},
  author = {Liu, Xinyu and Sai, Gaole and Duan, Shengyu},
  editor = {Liu, Shaoshan and Wei, Xiaohui},
  date = {2022},
  volume = {13615},
  pages = {192--204},
  publisher = {Springer Nature Switzerland},
  location = {Cham},
  doi = {10.1007/978-3-031-21395-3_18},
  url = {https://link.springer.com/10.1007/978-3-031-21395-3_18},
  urldate = {2025-05-16},
  isbn = {978-3-031-21394-6 978-3-031-21395-3},
  langid = {english}
}

@article{malekjafarian2019,
  title = {A {{Machine Learning Approach}} to {{Bridge-Damage Detection Using Responses Measured}} on a {{Passing Vehicle}}},
  author = {Malekjafarian, Abdollah and Golpayegani, Fatemeh and Moloney, Callum and Clarke, Siobhán},
  date = {2019-01},
  journaltitle = {Sensors},
  volume = {19},
  number = {18},
  pages = {4035},
  publisher = {Multidisciplinary Digital Publishing Institute},
  issn = {1424-8220},
  doi = {10.3390/s19184035},
  url = {https://www.mdpi.com/1424-8220/19/18/4035},
  urldate = {2024-04-02},
  abstract = {This paper proposes a new two-stage machine learning approach for bridge damage detection using the responses measured on a passing vehicle. In the first stage, an artificial neural network (ANN) is trained using the vehicle responses measured from multiple passes (training data set) over a healthy bridge. The vehicle acceleration or Discrete Fourier Transform (DFT) spectrum of the acceleration is used. The vehicle response is predicted from its speed for multiple passes (monitoring data set) over the bridge. Root-mean-square error is used to calculate the prediction error, which indicates the differences between the predicted and measured responses for each passage. In the second stage of the proposed method, a damage indicator is defined using a Gaussian process that detects the changes in the distribution of the prediction errors. It is suggested that if the bridge condition is healthy, the distribution of the prediction errors will remain low. A recognizable change in the distribution might indicate a damage in the bridge. The performance of the proposed approach was evaluated using numerical case studies of vehicle–bridge interaction. It was demonstrated that the approach could successfully detect the damage in the presence of road roughness profile and measurement noise, even for low damage levels.},
  issue = {18},
  langid = {english},
  keywords = {artificial neural network,bridge,damage detection,drive-by,machine learning},
  file = {C\:\\Users\\damar\\Zotero\\storage\\7WYKNBEK\\Malekjafarian et al. - 2019 - A Machine Learning Approach to Bridge-Damage Detec.pdf;C\:\\Users\\damar\\Zotero\\storage\\W9XNXSBP\\malekjafarian2019.pdf.pdf}
}

@article{mariani2024,
  title = {Data-Driven Modeling of Long Temperature Time-Series to Capture the Thermal Behavior of Bridges for {{SHM}} Purposes},
  author = {Mariani, S. and Kalantari, A. and Kromanis, R. and Marzani, A.},
  date = {2024-01-01},
  journaltitle = {Mechanical Systems and Signal Processing},
  shortjournal = {Mechanical Systems and Signal Processing},
  volume = {206},
  pages = {110934},
  issn = {0888-3270},
  doi = {10.1016/j.ymssp.2023.110934},
  url = {https://www.sciencedirect.com/science/article/pii/S0888327023008427},
  urldate = {2024-05-08},
  abstract = {Bridges experience complex heat propagation phenomena that are governed by external thermal loads, such as solar radiation and air convection, as well as internal factors, such as thermal inertia and geometrical properties of the various components. This dynamics produces internal temperature distributions which cause changes in some measurable structural responses that often surpass those produced by any other load acting on the structure or by the insurgence or growth of damage. This article advocates the use of regression models that are capable of capturing the dynamics buried within long sequences of temperature measurements and of relating that to some measured structural response, such as strain as in the test structure used in this study. Two such models are proposed, namely the multiple linear regression (MLR) and a deep learning (DL) method based on one-dimensional causal dilated convolutional neural networks, and their ability to predict strain is evaluated in terms of the coefficient of determination R2. Simple linear regression (LR), which only uses a single temperature reading to predict the structural response, is also tested and used as a benchmark. It is shown that both MLR and the DL method largely outperform LR, with the DL method providing the best results overall, though at a higher computational cost. These findings confirm the need to consider the evolution of temperature if one wishes to setup a temperature-based data-driven strategy for the SHM of large structures such as bridges, an example of which is given and discussed towards the end of the article.},
  keywords = {Bridges,Regression,SHM,Thermal inertia,Time-lag,WaveNet},
  file = {C:\Users\damar\Zotero\storage\CNNQXVU3\Mariani et al. - 2024 - Data-driven modeling of long temperature time-seri.pdf}
}

@article{melhem2003,
  title = {Damage {{Detection}} in {{Concrete}} by {{Fourier}} and {{Wavelet Analyses}}},
  author = {Melhem, Hani and Kim, Hansang},
  date = {2003-05-01},
  journaltitle = {Journal of Engineering Mechanics},
  volume = {129},
  number = {5},
  pages = {571--577},
  publisher = {American Society of Civil Engineers},
  issn = {0733-9399},
  doi = {10.1061/(ASCE)0733-9399(2003)129:5(571)},
  url = {https://ascelibrary.org/doi/10.1061/%28ASCE%290733-9399%282003%29129%3A5%28571%29},
  urldate = {2024-03-19},
  abstract = {The effectiveness of vibration-based methods in damage detection of a typical highway structure is investigated. Two types of full-scale concrete structures subjected to fatigue loads are studied: (1) Portland cement concrete pavements on grade; and (2) a ...},
  langid = {english},
  keywords = {concrete,Concrete structures,crack detection,Damage,dynamic response,fatigue,Fourier transform,Fourier transforms,nondestructive testing,Nondestructive tests,vibrations,wavelet transforms},
  file = {C:\Users\damar\Zotero\storage\6ZTIUGQL\melhem2003.pdf.pdf}
}

@article{miao2020,
  title = {A {{New Method}} of {{Denoising}} of {{Vibration Signal}} and {{Its Application}}},
  author = {Miao, Feng and Zhao, Rongzhen and Wang, Xianli},
  date = {2020-05-30},
  journaltitle = {Shock and Vibration},
  shortjournal = {Shock and Vibration},
  volume = {2020},
  pages = {1--8},
  issn = {1070-9622, 1875-9203},
  doi = {10.1155/2020/7587840},
  url = {https://www.hindawi.com/journals/sv/2020/7587840/},
  urldate = {2024-09-10},
  abstract = {In order to improve the performance of the denoising method for vibration signals of rotating machinery, a new method of signal denoising based on the improved median filter and wavelet packet technology is proposed through analysing the characteristics of noise components and relevant denoising methods. Firstly, the window width of the median filter is calculated according to the sampling frequency so that the impulse noise and part of the white noise can be effectively filtered out. Secondly, an improved self-adaptive wavelet packet denoising technique is used to remove the residual white noise. Finally, useful vibration signals are obtained after the previous processing. Simulation signals and rotor experimental vibration signals were used to verify the performance of the method. Experiment results show that the method can not only effectively eliminate the mixed complex noises but also preserve the fault character details, which demonstrates that the proposed method outperforms the method based on the wavelet-domain median filter.},
  langid = {english},
  file = {C\:\\Users\\damar\\Zotero\\storage\\LNJIL8MM\\miao2020.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\P8Z2YJPH\\Miao et al. - 2020 - A New Method of Denoising of Vibration Signal and .pdf}
}

@inproceedings{mironovova2015,
  title = {Fast Fourier Transform for Feature Extraction and Neural Network for Classification of Electrocardiogram Signals},
  booktitle = {2015 {{Fourth International Conference}} on {{Future Generation Communication Technology}} ({{FGCT}})},
  author = {Mironovova, Martina and Bíla, Jirí},
  date = {2015-07},
  pages = {1--6},
  issn = {2377-2638},
  doi = {10.1109/FGCT.2015.7300244},
  url = {https://ieeexplore.ieee.org/document/7300244},
  urldate = {2024-09-03},
  abstract = {This paper presents a novel approach to complex classification of heart abnormalities registered by electrocardiogram signals. It uses a combined approach of a Fast Fourier Technique for signal filtering and R-peaks detection and heart rate extraction, followed by signal modelling and classification by neural network based on recording of ECG. Obtained information is processed together for a complex evaluation of the signal in time.},
  eventtitle = {2015 {{Fourth International Conference}} on {{Future Generation Communication Technology}} ({{FGCT}})},
  keywords = {Data Filtering,Databases,Electrocardiogram Signal,Electrocardiography,Fast Fourier Transform,Heart beat,Heart rate variability,Neural Network,Neural networks,R-Peak Detection},
  file = {C\:\\Users\\damar\\Zotero\\storage\\KTRQVNQL\\mironovova2015.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\5Z2M5IAW\\7300244.html}
}

@article{nichols2004,
  title = {Use of Data-Driven Phase Space Models in Assessing the Strength of a Bolted Connection in a Composite Beam},
  author = {Nichols, J M and Nichols, C J and Todd, M D and Seaver, M and Trickey, S T and Virgin, L N},
  date = {2004-04-01},
  journaltitle = {Smart Materials and Structures},
  shortjournal = {Smart Mater. Struct.},
  volume = {13},
  number = {2},
  pages = {241--250},
  issn = {0964-1726, 1361-665X},
  doi = {10.1088/0964-1726/13/2/001},
  url = {https://iopscience.iop.org/article/10.1088/0964-1726/13/2/001},
  urldate = {2025-05-16}
}

@article{onchis2019,
  title = {A Deep Learning Approach to Condition Monitoring of Cantilever Beams via Time-Frequency Extended Signatures},
  author = {Onchis, Habil. Darian M.},
  date = {2019-02},
  journaltitle = {Computers in Industry},
  shortjournal = {Computers in Industry},
  volume = {105},
  pages = {177--181},
  issn = {01663615},
  doi = {10.1016/j.compind.2018.12.005},
  url = {https://linkinghub.elsevier.com/retrieve/pii/S0166361518305669},
  urldate = {2024-04-10},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\VMTHSXPK\37f540b431ff7b297a2ca5b8f2eb1454.pdf.pdf}
}

@article{pentaris2013,
  title = {A Novel Approach of {{Structural Health Monitoring}} by the Application of {{FFT}} and Wavelet Transform Using an Index of Frequency Dispersion},
  author = {Pentaris, Fragkiskos and Stonham, John and Makris, John},
  date = {2013-01-01},
  journaltitle = {International Journal of Geology},
  shortjournal = {International Journal of Geology},
  volume = {7},
  pages = {39--48},
  file = {C:\Users\damar\Zotero\storage\ADJEVL7C\Pentaris et al. - 2013 - A novel approach of Structural Health Monitoring b.pdf}
}

@article{rabi2024,
  title = {Effectiveness of {{Vibration-Based Techniques}} for {{Damage Localization}} and {{Lifetime Prediction}} in {{Structural Health Monitoring}} of {{Bridges}}: {{A Comprehensive Review}}},
  shorttitle = {Effectiveness of {{Vibration-Based Techniques}} for {{Damage Localization}} and {{Lifetime Prediction}} in {{Structural Health Monitoring}} of {{Bridges}}},
  author = {Rabi, Raihan Rahmat and Vailati, Marco and Monti, Giorgio},
  date = {2024-04},
  journaltitle = {Buildings},
  volume = {14},
  number = {4},
  pages = {1183},
  publisher = {Multidisciplinary Digital Publishing Institute},
  issn = {2075-5309},
  doi = {10.3390/buildings14041183},
  url = {https://www.mdpi.com/2075-5309/14/4/1183},
  urldate = {2024-05-07},
  abstract = {Bridges are essential to infrastructure and transportation networks, but face challenges from heavier traffic, higher speeds, and modifications like busway integration, leading to potential overloading and costly maintenance. Structural Health Monitoring (SHM) plays a crucial role in assessing bridge conditions and predicting failures to maintain structural integrity. Vibration-based condition monitoring employs non-destructive, in situ sensing and analysis of system dynamics across time, frequency, or modal domains. This method detects changes indicative of damage or deterioration, offering a proactive approach to maintenance in civil engineering. Such monitoring systems hold promise for optimizing the management and upkeep of modern infrastructure, potentially reducing operational costs. This paper aims to assist newcomers, practitioners, and researchers in navigating various methodologies for damage identification using sensor data from real structures. It offers a comprehensive review of prevalent anomaly detection approaches, spanning from traditional techniques to cutting-edge methods. Additionally, it addresses challenges inherent in Vibration-Based Damage (VBD) SHM applications, including establishing damage thresholds, corrosion detection, and sensor drift.},
  issue = {4},
  langid = {english},
  keywords = {challenges,damage thresholds,sensors,vibration-based SHM},
  file = {C:\Users\damar\Zotero\storage\2X8PMPF3\Rabi et al. - 2024 - Effectiveness of Vibration-Based Techniques for Da.pdf}
}

@article{rao2022,
  title = {A {{Novel Feature-Based SHM Assessment}} and {{Predication Approach}} for {{Robust Evaluation}} of {{Damage Data Diagnosis Systems}}},
  author = {Rao, M. Vishnu Vardhana and Chaparala, Aparna},
  date = {2022-06-01},
  journaltitle = {Wireless Personal Communications},
  shortjournal = {Wireless Pers Commun},
  volume = {124},
  number = {4},
  pages = {3387--3411},
  issn = {1572-834X},
  doi = {10.1007/s11277-022-09518-z},
  url = {https://doi.org/10.1007/s11277-022-09518-z},
  urldate = {2024-05-07},
  abstract = {Structural Health Monitoring (SHM) involves periodic recording and analysis in buildings and infrastructure prone to face external forces, ambient vibration, or natural climate changes. The sensors which are mounted on each floor capture the vibrations and create data with various features. SHM is vital in tracking the rate of deterioration of a structure and detecting damage, thereby maintaining safety. Feature selection, which indicates the process of choosing attributes in the dataset that can provide the best possible output accuracy, plays an important role in the analysis of a Damage Diagnosis system. The present paper proposes to use a combination of Mutual Information and Rough Set Theory for feature selection. After that, the paper proposes the hybrid technique of Support Vector Machine and Artificial Neural Network for increasing prediction accuracy. Comparison with various other commonly used techniques shows that the proposed approach provides a better classification accuracy.},
  langid = {english},
  keywords = {ANN (Artificial neural network),Data mining (DM),Feature selection (FS),Mutual information (MI),Neural networks (NN),Rough set theory (RST),SVM (Support vector machine)}
}

@inproceedings{rashinkar2017,
  title = {An Overview of Data Fusion Techniques},
  booktitle = {2017 {{International Conference}} on {{Innovative Mechanisms}} for {{Industry Applications}} ({{ICIMIA}})},
  author = {Rashinkar, Pratiksha and Krushnasamy, V. S.},
  date = {2017-02},
  pages = {694--697},
  doi = {10.1109/ICIMIA.2017.7975553},
  url = {https://ieeexplore.ieee.org/abstract/document/7975553/figures#figures},
  urldate = {2024-08-26},
  abstract = {Multi sensor data fusion is a tool used to combine the data from various sensors and gives a more reliable and accurate output. It is the integration of data and knowledge from several sources. This paper has reviewed the various technologies, the advantages and the classification of the data fusion.},
  eventtitle = {2017 {{International Conference}} on {{Innovative Mechanisms}} for {{Industry Applications}} ({{ICIMIA}})},
  keywords = {Data integration,Data models,Feature extraction,Industry applications,Process control,Robot sensing systems,Tutorials},
  file = {C\:\\Users\\damar\\Zotero\\storage\\XD9NDF48\\rashinkar2017.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\74DF6YBS\\figures.html}
}

@article{razi2013,
  title = {Improvement of a Vibration-Based Damage Detection Approach for Health Monitoring of Bolted Flange Joints in Pipelines},
  author = {Razi, Pejman and Esmaeel, Ramadan A and Taheri, Farid},
  date = {2013-05},
  journaltitle = {Structural Health Monitoring},
  shortjournal = {Structural Health Monitoring},
  volume = {12},
  number = {3},
  pages = {207--224},
  issn = {1475-9217, 1741-3168},
  doi = {10.1177/1475921713479641},
  url = {https://journals.sagepub.com/doi/10.1177/1475921713479641},
  urldate = {2025-05-16},
  abstract = {Early detection of bolt loosening is a major concern in the oil and gas industry. In this study, a vibration-based health monitoring strategy has been developed for detecting the loosening of bolts in a pipeline’s bolted flange joint. Both numerical and experimental studies are conducted to verify the integrity of our implementation as well as of an enhancement developed along with it. Several damage scenarios are simulated by the loosening of the bolts through varying the applied torque on each bolt. An electric impact hammer is used to vibrate (excite) the system in a consistent manner. The induced vibration signals are collected via piezoceramic sensors bonded onto the pipe and flange. These signals are transferred remotely by a wireless data acquisition module and then processed with a code developed in-house in the MATLAB environment. After normalization and filtering of the signals, the empirical mode decomposition is applied to establish an effective energy-based damage index. The assessment of the damage indices thus obtained for the various scenarios verifies the integrity of the proposed methodology for identifying the damage and its progression in bolted joints as well as the major enhancements applied onto the methodology.},
  langid = {english}
}

@inproceedings{sandirasegaram2005,
  title = {Comparative Analysis of Feature Extraction ({{2D FFT}} and Wavelet) and Classification ({{L}} p Metric Distances, {{MLP NN}}, and {{HNeT}}) Algorithms for {{SAR}} Imagery},
  author = {Sandirasegaram, Nicholas and English, Ryan},
  editor = {Zelnio, Edmund G. and Garber, Frederick D.},
  date = {2005-05-19},
  pages = {314},
  location = {Orlando, Florida, USA},
  doi = {10.1117/12.597305},
  url = {http://proceedings.spiedigitallibrary.org/proceeding.aspx?doi=10.1117/12.597305},
  urldate = {2024-09-03},
  eventtitle = {Defense and {{Security}}},
  file = {C:\Users\damar\Zotero\storage\GBAFVQY7\sandirasegaram2005.pdf.pdf}
}

@article{satpal2013,
  title = {Structural Health Monitoring of a Cantilever Beam Using Support Vector Machine},
  author = {Satpal, Satish B and Khandare, Yogesh and Guha, Anirban and Banerjee, Sauvik},
  date = {2013-12},
  journaltitle = {International Journal of Advanced Structural Engineering},
  shortjournal = {Int J Adv Struct Eng},
  volume = {5},
  number = {1},
  pages = {2},
  issn = {2008-3556, 2008-6695},
  doi = {10.1186/2008-6695-5-2},
  url = {https://link.springer.com/10.1186/2008-6695-5-2},
  urldate = {2024-04-02},
  abstract = {In this article, the effectiveness of support vector machine (SVM) is examined for health monitoring of beam-like structures using vibration-induced modal displacement data. The SVM is used to predict the intensity or location of damage in a simulated cantilever beam from displacements of the first mode shape. Twelve levels of damage intensities have been simulated at 12 locations, and six levels of white Gaussian noise have been added, thereby obtaining 1,008 simulations. About 90\% of these are used for training the SVM, and the remaining are used for testing. The trained SVM is able to predict damage intensity and location of all the training set data with nearly 100\% accuracy. The test set data reveal that SVM is able to predict damage intensity and damage location with errors varying from 0.28\% to 4.57\% and 0\% to 20.3\%, respectively, when there is no noise in the data. Addition of noise degrades the performance of SVM, the degradation being significant for intensity prediction and less for damage location prediction. The results demonstrate the use of SVM as a powerful tool for structural health monitoring without using the data of healthy state.},
  langid = {english},
  file = {C\:\\Users\\damar\\Zotero\\storage\\GBKEW3FA\\Satpal et al. - 2013 - Structural health monitoring of a cantilever beam .pdf;C\:\\Users\\damar\\Zotero\\storage\\LQ3G7S3Y\\satpal2013.pdf.pdf}
}

@inproceedings{shahid2022,
  title = {Performance {{Comparison}} of {{1D}} and {{2D Convolutional Neural Networks}} for {{Real-Time Classification}} of {{Time Series Sensor Data}}},
  booktitle = {2022 {{International Conference}} on {{Information Networking}} ({{ICOIN}})},
  author = {Shahid, Syed Maaz and Ko, Sunghoon and Kwon, Sungoh},
  date = {2022-01-12},
  pages = {507--511},
  publisher = {IEEE},
  location = {Jeju-si, Korea, Republic of},
  doi = {10.1109/ICOIN53446.2022.9687284},
  url = {https://ieeexplore.ieee.org/document/9687284/},
  urldate = {2025-05-16},
  eventtitle = {2022 {{International Conference}} on {{Information Networking}} ({{ICOIN}})},
  isbn = {978-1-66541-332-9}
}

@article{shang2021,
  title = {Vibration-Based Damage Detection for Bridges by Deep Convolutional Denoising Autoencoder},
  author = {Shang, Zhiqiang and Sun, Limin and Xia, Ye and Zhang, Wei},
  date = {2021-07-01},
  journaltitle = {Structural Health Monitoring},
  shortjournal = {Structural Health Monitoring},
  volume = {20},
  number = {4},
  pages = {1880--1903},
  publisher = {SAGE Publications},
  issn = {1475-9217},
  doi = {10.1177/1475921720942836},
  url = {https://doi.org/10.1177/1475921720942836},
  urldate = {2024-09-11},
  abstract = {One of the main challenges for structural damage detection using monitoring data is to acquire features that are sensitive to damages but insensitive to noise (e.g. sensor measurement noise) as well as environmental and operational effects (e.g. temperature effect). Inspired by the capabilities of deep learning methods in representation learning, various deep neural networks have been developed to obtain effective damage features from raw vibration data. However, most of the available deep neural networks are supervised, resulting in practical difficulties owing to the lack of damage labels. This article proposes a damage detection strategy based on an unsupervised deep neural network, referred to as deep convolutional denoising autoencoder, which accepts multi-dimensional cross-correlation functions as input. The strategy aims to extract damage features from field measurements of undamaged structures under the influence of noise and temperature uncertainties. In the proposed strategy, cross-correlation functions of vibration data are first calculated as basic features; then deep convolutional denoising autoencoder is developed to reconstruct cross-correlation functions from their noise-corrupted versions to extract desired features; exponentially weighted moving average control charts are finally established for these features to identify minor structural damages. The strategy is evaluated through a numerical simply supported beam model and an experimental continuous beam model. The mechanism of deep convolutional denoising autoencoder to extract damage features is interpreted by visualizing feature maps of convolutional layers in the encoder. It is found that these layers perform rough estimations of modal properties and preserve the damage information as the general trend of these properties in multiple extra frequency bands. The results show that the proposed strategy is competent for structural damage detection under the exposed environment and worth further exploring its capabilities in applications of real bridges.},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\2VCZ5JD7\10.1177@1475921720942836.pdf.pdf}
}

@article{shi2003,
  title = {Hilbert-Huang Transform and Wavelet Analysis of Time History Signal},
  author = {Shi, Chun-xiang and Luo, Qi-feng},
  date = {2003-07-01},
  journaltitle = {Acta Seismologica Sinica},
  shortjournal = {Acta Seimol. Sin.},
  volume = {16},
  number = {4},
  pages = {422--429},
  issn = {1993-1344},
  doi = {10.1007/s11589-003-0075-9},
  url = {https://doi.org/10.1007/s11589-003-0075-9},
  urldate = {2024-05-07},
  abstract = {The brief theories of wavelet analysis and Hilbert-Huang transform (HHT) are introduced firstly in the present paper. Then several signal data were analyzed by using wavelet and HHT methods, respectively. The comparison shows that HHT is not only an effective method for analyzing non-stationary data, but also is a useful tool for examining detailed characters of time history signal.},
  langid = {english},
  keywords = {Hilbert-Huang transform,intrinsic mode functions,mother wavelet,P315.63,spectral analysis,wavelet analysis},
  file = {C:\Users\damar\Zotero\storage\DCVA28MB\shi2003.pdf.pdf}
}

@article{tang2012,
  title = {Feature Extraction and Selection Based on Vibration Spectrum with Application to Estimating the Load Parameters of Ball Mill in Grinding Process},
  author = {Tang, Jian and Chai, Tianyou and Yu, Wen and Zhao, Lijie},
  date = {2012-10-01},
  journaltitle = {Control Engineering Practice},
  shortjournal = {Control Engineering Practice},
  series = {4th {{Symposium}} on {{Advanced Control}} of {{Industrial Processes}} ({{ADCONIP}})},
  volume = {20},
  number = {10},
  pages = {991--1004},
  issn = {0967-0661},
  doi = {10.1016/j.conengprac.2012.03.020},
  url = {https://www.sciencedirect.com/science/article/pii/S0967066112000846},
  urldate = {2024-09-03},
  abstract = {Feature extraction and selection are important issues in soft sensing and complex nonlinear system modeling. In this paper, a new feature extraction and selection approach based on the vibration frequency spectrum is proposed to estimate the load parameters of wet ball mill in grinding process. This approach can simplify the modeling process. In this study, the vibration acceleration signals are first transformed into the frequency spectrum by fast Fourier transform (FFT). Then the candidate features are extracted and selected from the frequency spectrum, which include characteristic frequency sub-bands, spectral principal components, and features of local peaks. Mutual information, spectral segment clustering and kernel principal component analysis are used to obtain these candidate features. Finally, a combinatorial optimization method based on adaptive genetic algorithm selects the input sub-set and parameters of the soft sensor model simultaneously. This approach is successfully applied in a laboratory scale wet ball mill. The test results show that the proposed approach is effective for modeling the parameters of mill load.},
  keywords = {Combinatorial optimization,Feature extraction,Feature selection,Frequency spectrum,Mill load,Soft sensor}
}

@article{toh2020,
  title = {Review of {{Vibration-Based Structural Health Monitoring Using Deep Learning}}},
  author = {Toh, Gyungmin and Park, Junhong},
  date = {2020-01},
  journaltitle = {Applied Sciences},
  volume = {10},
  number = {5},
  pages = {1680},
  publisher = {Multidisciplinary Digital Publishing Institute},
  issn = {2076-3417},
  doi = {10.3390/app10051680},
  url = {https://www.mdpi.com/2076-3417/10/5/1680},
  urldate = {2024-03-19},
  abstract = {With the rapid progress in the deep learning technology, it is being used for vibration-based structural health monitoring. When the vibration is used for extracting features for system diagnosis, it is important to correlate the measured signal to the current status of the structure. The measured vibration responses show large deviation in spectral and transient characteristics for systems to be monitored. Consequently, the diagnosis using vibration requires complete understanding of the extracted features to discard the influence of surrounding environments or unnecessary variations. The deep-learning-based algorithms are expected to find increasing application in these complex problems due to their flexibility and robustness. This review provides a summary of studies applying machine learning algorithms for fault monitoring. The vibration factors were used to categorize the studies. A brief interpretation of deep neural networks is provided to guide further applications in the structural vibration analysis.},
  issue = {5},
  langid = {english},
  keywords = {deep neural network,health monitoring,vibration},
  file = {C\:\\Users\\damar\\Zotero\\storage\\6XITVIKY\\toh2020.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\9L9KXB7V\\Toh and Park - 2020 - Review of Vibration-Based Structural Health Monito.pdf}
}

@article{vos2022,
  title = {Vibration-Based Anomaly Detection Using {{LSTM}}/{{SVM}} Approaches},
  author = {Vos, Kilian and Peng, Zhongxiao and Jenkins, Christopher and Shahriar, Md Rifat and Borghesani, Pietro and Wang, Wenyi},
  date = {2022-04},
  journaltitle = {Mechanical Systems and Signal Processing},
  shortjournal = {Mechanical Systems and Signal Processing},
  volume = {169},
  pages = {108752},
  issn = {08883270},
  doi = {10.1016/j.ymssp.2021.108752},
  url = {https://linkinghub.elsevier.com/retrieve/pii/S0888327021010682},
  urldate = {2024-03-18},
  langid = {english}
}

@article{wang2013,
  title = {Review of {{Bolted Connection Monitoring}}},
  author = {Wang, Tao and Song, Gangbing and Liu, Shaopeng and Li, Yourong and Xiao, Han},
  date = {2013-12-01},
  journaltitle = {International Journal of Distributed Sensor Networks},
  shortjournal = {International Journal of Distributed Sensor Networks},
  volume = {9},
  number = {12},
  pages = {871213},
  issn = {1550-1477, 1550-1477},
  doi = {10.1155/2013/871213},
  url = {http://journals.sagepub.com/doi/10.1155/2013/871213},
  urldate = {2025-05-16},
  abstract = {This paper reviews the research of monitoring technologies for bolted structural connections. The acoustoelastic effect based method, the piezoelectric active sensing method, and the piezoelectric impedance method are the three commonly used to monitor bolted connections. The basic principle and the applications of these three methods are discussed in detail in this paper. In addition, this paper presents a comparison of these methods and discusses their suitability for in situ or real-time bolt connection monitoring.},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\YVAKDMU9\wang2013.pdf.pdf}
}

@article{wang2016,
  title = {Damage Detection Using Frequency Shift Path},
  author = {Wang, Longqi and Lie, Seng Tjhen and Zhang, Yao},
  date = {2016-01-01},
  journaltitle = {Mechanical Systems and Signal Processing},
  shortjournal = {Mechanical Systems and Signal Processing},
  volume = {66--67},
  pages = {298--313},
  issn = {0888-3270},
  doi = {10.1016/j.ymssp.2015.06.028},
  url = {https://www.sciencedirect.com/science/article/pii/S0888327015003167},
  urldate = {2024-05-07},
  abstract = {This paper introduces a novel concept called FREquency Shift (FRESH) path to describe the dynamic behavior of structures with auxiliary mass. FRESH path combines the effects of frequency shifting and amplitude changing into one space curve, providing a tool for analyzing structure health status and properties. A damage index called FRESH curvature is then proposed to detect local stiffness reduction. FRESH curvature can be easily adapted for a particular problem since the sensitivity of the index can be adjusted by changing auxiliary mass or excitation power. An algorithm is proposed to adjust automatically the contribution from frequency and amplitude in the method. Because the extraction of FRESH path requires highly accurate frequency and amplitude estimators; therefore, a procedure based on discrete time Fourier transform is introduced to extract accurate frequency and amplitude with the time complexity of O(nlogn), which is verified by simulation signals. Moreover, numerical examples with different damage sizes, severities and damping are presented to demonstrate the validity of the proposed damage index. In addition, applications of FRESH path on two steel beams with different damages are presented and the results show that the proposed method is valid and computational efficient.},
  keywords = {Auxiliary mass,Damage detection,Discrete time Fourier transform,Frequency shift path},
  file = {C:\Users\damar\Zotero\storage\8KYYV56B\wang2016.pdf.pdf}
}

@incollection{wanhammar1999,
  title = {Digital {{Signal Processing}}},
  booktitle = {{{DSP Integrated Circuits}}},
  author = {Wanhammar, Lars},
  date = {1999},
  pages = {59--114},
  publisher = {Elsevier},
  doi = {10.1016/B978-012734530-7/50003-9},
  url = {https://linkinghub.elsevier.com/retrieve/pii/B9780127345307500039},
  urldate = {2024-03-18},
  isbn = {978-0-12-734530-7},
  langid = {english}
}

@article{widodo2007,
  title = {Support Vector Machine in Machine Condition Monitoring and Fault Diagnosis},
  author = {Widodo, Achmad and Yang, Bo-Suk},
  date = {2007-08-01},
  journaltitle = {Mechanical Systems and Signal Processing},
  shortjournal = {Mechanical Systems and Signal Processing},
  volume = {21},
  number = {6},
  pages = {2560--2574},
  issn = {0888-3270},
  doi = {10.1016/j.ymssp.2006.12.007},
  url = {https://www.sciencedirect.com/science/article/pii/S0888327007000027},
  urldate = {2024-09-08},
  abstract = {Recently, the issue of machine condition monitoring and fault diagnosis as a part of maintenance system became global due to the potential advantages to be gained from reduced maintenance costs, improved productivity and increased machine availability. This paper presents a survey of machine condition monitoring and fault diagnosis using support vector machine (SVM). It attempts to summarize and review the recent research and developments of SVM in machine condition monitoring and diagnosis. Numerous methods have been developed based on intelligent systems such as artificial neural network, fuzzy expert system, condition-based reasoning, random forest, etc. However, the use of SVM for machine condition monitoring and fault diagnosis is still rare. SVM has excellent performance in generalization so it can produce high accuracy in classification for machine condition monitoring and diagnosis. Until 2006, the use of SVM in machine condition monitoring and fault diagnosis is tending to develop towards expertise orientation and problem-oriented domain. Finally, the ability to continually change and obtain a novel idea for machine condition monitoring and fault diagnosis using SVM will be future works.},
  keywords = {Fault diagnosis,Machine condition monitoring,Support vector machine},
  file = {C:\Users\damar\Zotero\storage\KGSTJGAQ\widodo2007.pdf.pdf}
}

@article{pham2020,
  title = {Bolt-{{Loosening Monitoring Framework Using}} an {{Image-Based Deep Learning}} and {{Graphical Model}}},
  author = {Pham, Hai Chien and Ta, Quoc-Bao and Kim, Jeong-Tae and Ho, Duc-Duy and Tran, Xuan-Linh and Huynh, Thanh-Canh},
  date = {2020-06-15},
  journaltitle = {Sensors},
  shortjournal = {Sensors},
  volume = {20},
  number = {12},
  pages = {3382},
  issn = {1424-8220},
  doi = {10.3390/s20123382},
  url = {https://www.mdpi.com/1424-8220/20/12/3382},
  urldate = {2025-05-16},
  abstract = {In this study, we investigate a novel idea of using synthetic images of bolts which are generated from a graphical model to train a deep learning model for loosened bolt detection. Firstly, a framework for bolt-loosening detection using image-based deep learning and computer graphics is proposed. Next, the feasibility of the proposed framework is demonstrated through the bolt-loosening monitoring of a lab-scaled bolted joint model. For practicality, the proposed idea is evaluated on the real-scale bolted connections of a historical truss bridge in Danang, Vietnam. The results show that the deep learning model trained by the synthesized images can achieve accurate bolt recognitions and looseness detections. The proposed methodology could help to reduce the time and cost associated with the collection of high-quality training data and further accelerate the applicability of vision-based deep learning models trained on synthetic data in practice.},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\H59BPKEK\10.3390@s20123382.pdf.pdf}
}

@article{garrido2016,
  title = {The {{Feedforward Short-Time Fourier Transform}}},
  author = {Garrido, Mario},
  date = {2016-09},
  journaltitle = {IEEE Transactions on Circuits and Systems II: Express Briefs},
  shortjournal = {IEEE Trans. Circuits Syst. II},
  volume = {63},
  number = {9},
  pages = {868--872},
  issn = {1549-7747, 1558-3791},
  doi = {10.1109/TCSII.2016.2534838},
  url = {http://ieeexplore.ieee.org/document/7419878/},
  urldate = {2025-05-16},
  file = {C\:\\Users\\damar\\Zotero\\storage\\RD6LN5MR\\Garrido - 2016 - The Feedforward Short-Time Fourier Transform.pdf;C\:\\Users\\damar\\Zotero\\storage\\X8TBD546\\garrido2016.pdf.pdf}
}

@article{zhang2023,
  title = {Signal {{Enhancement Methods Based}} on {{Wavelet Transform}}, {{Fractional Fourier Transform}} and {{Short-time Fourier Transform}}},
  author = {Zhang, Xindan and Zheng, Haoyuan},
  date = {2023-12-31},
  journaltitle = {Highlights in Science, Engineering and Technology},
  shortjournal = {HSET},
  volume = {76},
  pages = {222--230},
  issn = {2791-0210},
  doi = {10.54097/eyfndn07},
  url = {https://drpress.org/ojs/index.php/HSET/article/view/15890},
  urldate = {2025-05-16},
  abstract = {This review paper mainly focuses on different signal enhancement methods such as wavelet transform, fractional Fourier transform (FrFT) and short-time Fourier transform (STFT). First, this paper introduces the concept and importance of signal enhancement, as well as some current issues and challenges. Then, in recent years, the application of the three methods in wavelet transform, fractional Fourier transform and short-time Fourier transform is described. In terms of wavelet transform, this paper discusses the application of wavelet function to image enhancement and the specific steps, and analyzes its advantages and application in signal enhancement. In terms of fractional Fourier transform, this paper introduces its difference from traditional Fourier transform, and discusses its application in combination with adaptive filtering technology and the application of multi-level FrFT in the field of speech enhancement. Finally, in terms of short-time Fourier transform, this paper discusses its application in the fields of image enhancement and speech enhancement. The review paper finally discusses the characteristics, advantages and limitations of these three methods in signal enhancement, and looks forward to the future research directions. Through the research of this review paper, it can provide some reference and guidance for the research in the field of signal enhancement.}
}

@article{kong2018,
  title = {Tapping and Listening: A New Approach to Bolt Looseness Monitoring},
  shorttitle = {Tapping and Listening},
  author = {Kong, Qingzhao and Zhu, Junxiao and Ho, Siu Chun Michael and Song, Gangbing},
  date = {2018-07-01},
  journaltitle = {Smart Materials and Structures},
  shortjournal = {Smart Mater. Struct.},
  volume = {27},
  number = {7},
  pages = {07LT02},
  issn = {0964-1726, 1361-665X},
  doi = {10.1088/1361-665X/aac962},
  url = {https://iopscience.iop.org/article/10.1088/1361-665X/aac962},
  urldate = {2025-05-16},
  file = {C:\Users\damar\Zotero\storage\VR74RNZF\kong2018.pdf.pdf}
}

@article{wu2020,
  title = {Data Fusion Approaches for Structural Health Monitoring and System Identification: {{Past}}, Present, and Future},
  shorttitle = {Data Fusion Approaches for Structural Health Monitoring and System Identification},
  author = {Wu, Rih-Teng and Jahanshahi, Mohammad Reza},
  date = {2020-03-01},
  journaltitle = {Structural Health Monitoring},
  shortjournal = {Structural Health Monitoring},
  volume = {19},
  number = {2},
  pages = {552--586},
  publisher = {SAGE Publications},
  issn = {1475-9217},
  doi = {10.1177/1475921718798769},
  url = {https://doi.org/10.1177/1475921718798769},
  urldate = {2024-05-07},
  abstract = {During the past decades, significant efforts have been dedicated to develop reliable methods in structural health monitoring. The health assessment for the target structure of interest is achieved through the interpretation of collected data. At the beginning of the 21st century, the rapid advances in sensor technologies and data acquisition platforms have led to the new era of Big Data, where a huge amount of heterogeneous data are collected by a variety of sensors. The increasing accessibility and diversity of the data resources provide new opportunities for structural health monitoring, while the aggregation of information obtained from multiple sensors to make robust decisions remains a challenging problem. This article presents a comprehensive review of the recent data fusion applications in structural health monitoring. State-of-the-art theoretical concepts and applications of data fusion in structural health monitoring are presented. Challenges for data fusion in structural health monitoring are discussed, and a roadmap is provided for future research in this area.},
  langid = {english}
}

@article{yang2020,
  title = {Data-{{Driven Feature Extraction}} for {{Analog Circuit Fault Diagnosis Using}} 1-{{D Convolutional Neural Network}}},
  author = {Yang, Huahui and Meng, Chen and Wang, Cheng},
  date = {2020},
  journaltitle = {IEEE Access},
  shortjournal = {IEEE Access},
  volume = {8},
  pages = {18305--18315},
  issn = {2169-3536},
  doi = {10.1109/ACCESS.2020.2968744},
  url = {https://ieeexplore.ieee.org/document/8966245/},
  urldate = {2025-05-16},
  file = {C:\Users\damar\Zotero\storage\3FYS28EI\Yang et al. - 2020 - Data-Driven Feature Extraction for Analog Circuit .pdf}
}

@article{yin2018,
  title = {Probabilistic {{Damage Detection}} of a {{Steel Truss Bridge Model}} by {{Optimally Designed Bayesian Neural Network}}},
  author = {Yin, Tao and Zhu, Hong-ping},
  date = {2018-10-09},
  journaltitle = {Sensors},
  shortjournal = {Sensors},
  volume = {18},
  number = {10},
  pages = {3371},
  issn = {1424-8220},
  doi = {10.3390/s18103371},
  url = {https://www.mdpi.com/1424-8220/18/10/3371},
  urldate = {2024-12-29},
  abstract = {Excellent pattern matching capability makes artificial neural networks (ANNs) a very promising approach for vibration-based structural health monitoring (SHM). The proper design of the network architecture with the suitable complexity is vital to the ANN-based structural damage detection. In addition to the number of hidden neurons, the type of transfer function used in the hidden layer cannot be neglected for the ANN design. Neural network learning can be further presented in the framework of Bayesian statistics, but the issues of selection for the hidden layer transfer function with respect to the Bayesian neural network has not yet been reported in the literature. In addition, most of the research works in the literature for addressing the predictive distribution of neural network output is only for a single target variable, while multiple target variables are rarely involved. In the present paper, for the purpose of probabilistic structural damage detection, Bayesian neural networks with multiple target variables are optimally designed, and the selection of the number of neurons, and the transfer function in the hidden layer, are carried out simultaneously to achieve a neural network architecture with suitable complexity. Furthermore, the nonlinear network function can be approximately linear by assuming the posterior distribution of network parameters is a sufficiently narrow Gaussian, and then the input-dependent covariance matrix of the predictive distribution of network output can be obtained with the Gaussian assumption for the situation of multiple target variables. Structural damage detection is conducted for a steel truss bridge model to verify the proposed method through a set of numerical case studies.},
  langid = {english},
  file = {C:\Users\damar\Zotero\storage\9K8YXV76\a1274f7304475ebcd1c70132b01411b0.pdf.pdf}
}

@inproceedings{yumang2020,
  title = {Combination of {{Acoustic}} and {{Vibration Sensor Data Using Support Vector Machines}} and {{One-Versus-All Technique Data Fusion}} for {{Detecting Objects}}},
  booktitle = {Proceedings of the 2020 12th {{International Conference}} on {{Computer}} and {{Automation Engineering}}},
  author = {Yumang, Analyn N. and Cruz, Geriel Angelo and Fontanilla, Llanz Adeo},
  date = {2020-05-16},
  series = {{{ICCAE}} 2020},
  pages = {56--59},
  publisher = {Association for Computing Machinery},
  location = {New York, NY, USA},
  doi = {10.1145/3384613.3384626},
  url = {https://doi.org/10.1145/3384613.3384626},
  urldate = {2024-08-26},
  abstract = {This paper aims to create a device that will be able to detect the presence of an object and classify the object into human, animal, or vehicle by using the information obtained from acoustic and seismic signals. The specific objectives are to develop a hardware device based from Raspberry Pi Minicomputer with seismic and acoustic sensors and transmit sensor signals to a computer for feature extraction and data fusion, to develop a software using Python, MATLAB, and use Data Fusion with the use of Support Vector Machine with One-Versus-All technique, to accurately classify the object into human, animal (canine), or vehicle, to use statistical treatment using multi-class confusion matrix to determine the F-score or accuracy of the classifiers, as an aid for answering the formulated hypotheses. In the testing phase, blind test was performed for the classifiers, using different gathered samples. The F-score of the human, animal, and vehicle classifiers were, respectively, 93.549\%, 98.305\%, and 100\%. The researchers recommend a ground-mounted seismic sensor for comparison of its F-score contribution with the used seismic sensor. Training the SVM models with different parameters could also lead to potential increase in accuracy, such as the number of k-fold cross validations. SVM can as well be compared to other classifier models.},
  isbn = {978-1-4503-7678-5},
  file = {C:\Users\damar\Zotero\storage\M6RVFMLR\yumang2020.pdf.pdf}
}

@article{zhan2021,
  title = {A {{Step-by-Step Damage Identification Method Based}} on {{Frequency Response Function}} and {{Cross Signature Assurance Criterion}}},
  author = {Zhan, Jiawang and Zhang, Fei and Siahkouhi, Mohammad},
  date = {2021-02-03},
  journaltitle = {Sensors},
  shortjournal = {Sensors},
  volume = {21},
  number = {4},
  pages = {1029},
  issn = {1424-8220},
  doi = {10.3390/s21041029},
  url = {https://www.mdpi.com/1424-8220/21/4/1029},
  urldate = {2024-12-29},
  abstract = {This paper aims to present a method for quantitative damage identification of a simply supported beam, which integrates the frequency response function (FRF) and model updating. The objective function is established using the cross-signature assurance criterion (CSAC) indices of the FRFs between the measurement points and the natural frequency. The CSAC index in the frequency range between the first two frequencies is found to be sensitive to damage. The proposed identification procedure is tried to identify the single and multiple damages. To verify the effectiveness of the method, numerical simulation and laboratory testing were conducted on some model steel beams with simulated damage by cross-cut sections, and the identification results were compared with the real ones. The analysis results show that the proposed damage evaluation method is insensitive to the systematic test errors and is able to locate and quantify the damage within the beam structures step by step.},
  langid = {english},
  file = {C\:\\Users\\damar\\Zotero\\storage\\3UBKNCJL\\zhan2021.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\IFFPNAQV\\Zhan et al. - 2021 - A Step-by-Step Damage Identification Method Based .pdf}
}

@article{zhang2020,
  title = {Autonomous Bolt Loosening Detection Using Deep Learning},
  author = {Zhang, Yang and Sun, Xiaowei and Loh, Kenneth J and Su, Wensheng and Xue, Zhigang and Zhao, Xuefeng},
  date = {2020-01},
  journaltitle = {Structural Health Monitoring},
  shortjournal = {Structural Health Monitoring},
  volume = {19},
  number = {1},
  pages = {105--122},
  issn = {1475-9217, 1741-3168},
  doi = {10.1177/1475921719837509},
  url = {https://journals.sagepub.com/doi/10.1177/1475921719837509},
  urldate = {2025-05-16},
  abstract = {Machine vision-based structural health monitoring is gaining popularity due to the rich information one can extract from video and images. However, the extraction of characteristic parameters from images often requires manual intervention, thereby limiting its scalability and effectiveness. In contrast, deep learning overcomes the aforementioned shortcoming in that it can autonomously extract feature parameters (e.g. structural damage) from image datasets. Therefore, this study aims to validate the use of machine vision and deep learning for structural health monitoring by focusing on a particular application of detecting bolt loosening. First, a dataset that contains 300 images was collected. The dataset includes two bolt states, namely, tight and loosened. Second, a faster region-based convolutional neural network was trained and evaluated. The test results showed that the average precision of bolt damage detection is 0.9503. Thereafter, bolts were loosened to various screw heights, and images obtained from different angles, lighting conditions, and vibration conditions were identified separately. The trained model was then employed to validate that bolt loosening could be detected with sufficient accuracy using various types of images. Finally, the trained model was connected with a webcam to realize real-time bolt loosening damage monitoring.},
  langid = {english},
  file = {C\:\\Users\\damar\\Zotero\\storage\\4W5HFTDL\\Zhang et al. - 2020 - Autonomous bolt loosening detection using deep lea.pdf;C\:\\Users\\damar\\Zotero\\storage\\C7HSH97N\\10.1177@1475921719837509.pdf.pdf}
}

@article{zhang2020a,
  title = {Autonomous Bolt Loosening Detection Using Deep Learning},
  author = {Zhang, Yang and Sun, Xiaowei and Loh, Kenneth J and Su, Wensheng and Xue, Zhigang and Zhao, Xuefeng},
  date = {2020-01},
  journaltitle = {Structural Health Monitoring},
  shortjournal = {Structural Health Monitoring},
  volume = {19},
  number = {1},
  pages = {105--122},
  issn = {1475-9217, 1741-3168},
  doi = {10.1177/1475921719837509},
  url = {https://journals.sagepub.com/doi/10.1177/1475921719837509},
  urldate = {2025-05-16},
  abstract = {Machine vision-based structural health monitoring is gaining popularity due to the rich information one can extract from video and images. However, the extraction of characteristic parameters from images often requires manual intervention, thereby limiting its scalability and effectiveness. In contrast, deep learning overcomes the aforementioned shortcoming in that it can autonomously extract feature parameters (e.g. structural damage) from image datasets. Therefore, this study aims to validate the use of machine vision and deep learning for structural health monitoring by focusing on a particular application of detecting bolt loosening. First, a dataset that contains 300 images was collected. The dataset includes two bolt states, namely, tight and loosened. Second, a faster region-based convolutional neural network was trained and evaluated. The test results showed that the average precision of bolt damage detection is 0.9503. Thereafter, bolts were loosened to various screw heights, and images obtained from different angles, lighting conditions, and vibration conditions were identified separately. The trained model was then employed to validate that bolt loosening could be detected with sufficient accuracy using various types of images. Finally, the trained model was connected with a webcam to realize real-time bolt loosening damage monitoring.},
  langid = {english},
  file = {C\:\\Users\\damar\\Zotero\\storage\\PC2JD3K8\\10.1177@1475921719837509.pdf.pdf;C\:\\Users\\damar\\Zotero\\storage\\Y98JZ4NQ\\Zhang et al. - 2020 - Autonomous bolt loosening detection using deep lea.pdf}
}

@online{zotero-437,
  title = {Scipy.Fft.Fft — {{SciPy}} v1.13.0 {{Manual}}},
  url = {https://docs.scipy.org/doc/scipy/reference/generated/scipy.fft.fft.html},
  urldate = {2024-05-07}
}

@thesis{zotero-622,
  type = {thesis}
}

@thesis{rytter1993,
  title = {Vibrational {{Based Inspection}} of {{Civil Engineering Structures}}},
  author = {Rytter, Anders},
  date = {1993},
  institution = {Aalborg University},
  location = {Aalborg},
  url = {https://vbn.aau.dk/en/publications/vibrational-based-inspection-of-civil-engineering-structures},
  abstract = {The thesis has been written in relation to two different research projects. Firstly, an offshore test programme, Integrated Experimental/Numerical Analysis of the Dynamic behavior  of offshore structures, which was performed at the department of Building Technology and Structural Engineering at the University of Aalborg from 1988 to 1991. Secondly, a research project, In-Field Vibration Based Inspection of Civil Engineering Structures, which has been performed as a pilot project by the Consulting Engineers Rambøll, Hannemann and Højlund in cooperation with the department of Building Technology and Structural Engineering at the University of Aalborg since the beginning of 1992. Both projects have been supported by the Danish Technical Research Council. Further, the first mentioned project was supported by the Danish Energy Agency. Their financial support is gratefully acknowledged.},
  langid = {english},
  keywords = {Beam,Bridges,Cracks,Damping,Offshore Platform,Piles,Structural Damage,VBI,Vibration Based Inspection}
}
